﻿int redMain = 2;﻿int yellowMain = 3;﻿int greenMain = 4;﻿int redSide = 5;﻿int yellowSide = 6;﻿int greenSide = 7;﻿void setup() {﻿  pinMode(redMain, OUTPUT);﻿  pinMode(yellowMain, OUTPUT);﻿  pinMode(greenMain, OUTPUT);

* pinMode(redSide, OUTPUT);

  pinMode(yellowSide, OUTPUT);﻿  pinMode(greenSide, OUTPUT);﻿}﻿void loop() ﻿  digitalWrite(greenMain, HIGH);﻿  digitalWrite(redSide, HIGH);﻿  delay(5000); ﻿  digitalWrite(yellowMain, HIGH);﻿  delay(2000); ﻿  digitalWrite(greenMain, LOW);﻿  digitalWrite(yellowMain, LOW);﻿  digitalWrite(redMain, HIGH);﻿﻿  digitalWrite(greenSide, HIGH);﻿  delay(5000); ﻿﻿  digitalWrite(yellowSide, HIGH);﻿  delay(2000); ﻿﻿  digitalWrite(greenSide, LOW);﻿  digitalWrite(yellowSide, LOW);﻿  digitalWrite(redSide, HIGH);﻿  delay(1000);﻿}